

Fig.4. Plot of first peak current (ip) versus concentration of (E)-1-(furan-2-yl)-3-

phenylprop-2-ene-1-ones in tetra butyl ammonium tetra fluoroborate.

Solvent = acetonitrile; Sweep rate = 40 mV/s